COMGOYÁ
TECHNICAL RIDER
International Cuban Orchestra
Comgoyá is an 11-piece International Cuban Orchestra performing Afro-Cuban and Cuban music. This rider describes the standard technical requirements for the ensemble. Requirements may be adapted by prior agreement.
	Booking / production
	Sissel Jor · Cuban Music
+47 99 49 62 88 · sjor@cubanmusic.no

	Musical director
	Felix Navarro Navarro
+47 93 94 73 65 · comgoyanavarro@yahoo.es


Load-in & soundcheck
Please allow 1–2 hours for load-in, line check and soundcheck, provided that PA, backline and stage power are ready on arrival. Final timings are agreed with the promoter.
Line-up & microphone / DI overview
	Musician
	Instrument / role
	Mic / DI

	Felix Navarro Navarro
	Congas, batá
	Instrument microphones

	Norge Flores Falcón
	Lead vocals
	Vocal microphone

	Rayner Tarín Camps
	Lead vocals
	Vocal microphone

	Antonio Torner
	Timbales
	Instrument microphones

	Jason Storsve
	Bass
	DI / bass amplifier

	Jomar Cabrera Reyes
	Lead vocals
	Vocal microphone

	Katerine Espinal
	Piano / keyboard
	DI

	Valerio Bottari
	Guitar / Cuban tres, backing vocals
	DI + vocal microphone

	Brage Rognlien
	Trombone
	Instrument microphone

	Kim L. Koffeld
	Trumpet
	Instrument microphone

	Alejandra Tabita
	Lead vocals
	Vocal microphone


Backline & instruments
Comgoyá brings its own personal instruments. The following backline is requested from the venue, subject to advance agreement:
Bass amplifier
Piano or suitable keyboard
Music stands as required
Required drum/percussion hardware and other standard backline agreed in advance.
Stage layout
The stage layout is adapted to the size of the stage. As a general rule, bass, timbales and congas are positioned at the rear, with piano/keyboard, guitar/tres and brass in the front or middle area. The four lead vocalists are positioned across the front of the stage. Final placement is agreed with the promoter and local technical crew. Please refer to the separate stage plot if supplied.
Technical requirements
Microphones
5 vocal microphones: four lead vocalists + backing vocal (guitar/tres).
2 instrument microphones for brass: trumpet and trombone.
2 instrument microphones for congas.
2 instrument microphones for timbales and/or cymbals.
Direct inputs (DI)
3 DI boxes for keyboard/piano, guitar and Cuban tres.
Bass via DI and/or bass amplifier, to be agreed with the local sound engineer.
Monitoring
6–7 stage monitors with sufficient separate monitor mixes for the ensemble.
PA / additional
A professional PA system suitable for the venue, with sufficient channels for the input requirements above.
Comgoyá carries a Zoom H4n Pro and, where practical and agreed with the engineer, would like to record a stereo feed from the mixing console.
DJ connection (when applicable)
For events that include a DJ, the DJ controller must be connectable to the mixer/PA. The exact connection (e.g. RCA/phono, jack or other line-level output) should be agreed in advance.
Communication
Please contact us as early as possible if any requirement is unclear or cannot be met. We are happy to work with the venue’s technical team to find practical solutions.
www.comgoya.no
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